#
SIDE SILL PANEL REMOVAL

BHE098070270B03

1. Rough cut area (A) and drill the 110 weld locations indicated by (B), then remove the side sill outer.

  Caution

  • Avoid cutting with a blowtorch or similar tools as the insulator (shaded area) is flammable.

2. Rough cut area (C) and drill the 40 weld locations indicated by (D), then remove the side sill reinforcement.

3. Remove the side sill rear reinforcement.