#
TRANSMISSION OIL REPLACEMENT [Y16M-D]

BHE051127001W04

1. Position the vehicle on level ground.

2. Remove oil filler plug and drain plug, and then drain the oil.

3. Clean drain plug.

4. Install drain plug and a new washer.

  Tightening torque
  27-48 N·m {2.8-4.9 kgf·m, 20-35 ft·lbf}

5. Add the specified amount and type of oil through the plug port for oil filler plug to near the brim of the port.

  Specified oil grade
  API Service GL-4 or GL-5
  Specified oil viscosity
  SAE 75W-90
  Capacity (approx. quantity)
  1.75 L {1.85 US qt, 1.54 lmp qt}

6. Install oil filler plug and a new washer.

  Tightening torque
  27-48 N·m {2.8-4.9 kgf·m, 20-35 ft·lbf}