#
NO.24 A/C IS ALWAYS ON OR A/C COMPRESSOR RUNS CONTINUOUSLY

BHE010300103W26

24 | A/C IS ALWAYS ON OR A/C COMPRESSOR RUNS CONTINUOUSLY.
--- | ---
DESCRIPTION | The A/C compressor magnetic clutch does not disengage.
POSSIBLE CAUSE | • Stuck engagement A/C compressor magnetic clutch • A/C relay is stuck closed. • Short to GND between A/C switch and PCM • Short to GND circuit between A/C relay and PCM • A/C relay to magnetic clutch circuit shorted to battery power

Diagnostic procedure

STEP | INSPECTION | RESULTS | ACTION
--- | --- | --- | ---
1 | Connect the WDS or equivalent to the DLC-2. Retrieve any continuous memory, KOEO and KOER DTCs. Are there any DTCs displayed? | Yes | DTC is displayed: Go to the applicable DTC inspection. (See DTC TABLE.)
No | No DTC is displayed: Go to the next step.
2 | Start the engine and run it at idle. Turn the A/C switch on. Remove the A/C relay. Does the A/C magnetic clutch disengage? | Yes | Inspect for the following: • The A/C relay is stuck closed. • Short to GND circuit between the A/C relay and PCM terminal 5AA. If both items normal, go to the next step.
No | Inspect if the circuit between the A/C relay and the magnetic clutch shorts to the battery power circuit. If the circuit is normal, inspect the magnetic clutch for stuck engagement or clearance.
3 | Connect the WDS or equivalent to the DLC-2. Access the ACSW PID. Start the engine and turn the A/C switch on. Read the ACSW PID while disconnecting the refrigerant pressure switch connector. Note • The ACSW PID should indicate that it is off when disconnecting the connector. If the ACSW PID remains on, a short to GND circuit may be present. Does the ACSW PID remain on? | Yes | Inspect for short to GND circuit between refrigerant pressure switch and PCM terminal 4W.
No | Go to the next step.
4 | Reconnect the refrigerant pressure switch connector. Read the ACSW PID while turning off the A/C switch. Note • The ACSW PID should indicate that it is off when turning the A/C switch off. If the ACSW PID remains on, a short to GND circuit may be present. Does the ACSW PID remain on? | Yes | Inspect the following: • Short to GND circuit between A/C switch and A/C amplifier • Short to GND circuit between A/C amplifier and refrigerant pressure switch
No | Inspect for stuck closed A/C switch.
5 | Verify test results. • If normal, return to the diagnostic index to service any additional symptoms. • If the malfunction remains, inspect the related Service Information and perform the repair or diagnosis.