#
CLUTCH HOUSING AND EXTENSION HOUSING INSPECTION

BHE051117010M02

## Shift Rod End, Control Rod

1. Measure the clearance between the shift rod end and control rod using a feeler gauge.

  • If not within the specification, replace the shift rod end and control rod as a set.

  Standard
  0.8 mm {0.031 in} or less

## Spring

1. Measure the free length of the spring.

  • If not within the specification, replace the spring.

  Standard
mm {in}

| 13B-MSP | 13B-Turbo
Select lock spindle spring | 75.1 {2.957} | 43.25 {1.703}