#
DTC P0138

BHE010200100W18

DTC P0138 | Rear HO2S circuit high voltage
--- | ---
DETECTION CONDITION | • The PCM monitors the input voltage from the rear HO2S when the engine is running. If the input voltage is more than 1.2 V, the PCM determines that the rear HO2S circuit voltage is high. Diagnostic support note • This is an intermittent monitor (HO2S). • The MIL illuminates if the PCM detects the above malfunction condition in two consecutive drive cycles or in one drive cycle while the DTC for the same malfunction has been stored in the PCM. • PENDING CODE is available if the PCM detects the above malfunction condition during the first drive cycle. • FREEZE FRAME DATA is available. • The DTC is stored in the PCM memory.
POSSIBLE CAUSE | • Rear HO2S malfunction • Connector or terminal malfunction • Short to power supply in wiring harness between rear HO2S terminal A and PCM terminal 2Q • PCM malfunction

Diagnostic procedure

STEP | INSPECTION | ACTION
--- | --- | ---
1 | VERIFY FREEZE FRAME DATA HAS BEEN RECORDED • Has FREEZE FRAME DATA been recorded? | Yes | Go to the next step.
No | Record the FREEZE FRAME DATA on the repair order, then go to the next step.
2 | VERIFY RELATED REPAIR INFORMATION AVAILABILITY • Verify related service repair information availability. • Is any related repair information available? | Yes | Perform repair or diagnosis according to the available repair information. • If the vehicle is not repaired, go to the next step.
No | Go to the next step.
3 | INSPECT REAR HO2S CONNECTOR FOR POOR CONNECTION • Turn the ignition switch off. • Disconnect the rear HO2S connector. • Inspect for poor connection (such as damaged/pulled-out pins, corrosion). • Is there any malfunction? | Yes | Repair or replace the terminal, then go to Step 7.
No | Go to the next step.
4 | INSPECT REAR HO2S CIRCUIT FOR SHORT TO POWER SUPPLY • Turn the ignition switch to the ON position (Engine off). • Measure the voltage between rear HO2S terminal A (wiring harness-side) and body GND. • Is the voltage B+? | Yes | Repair or replace the wiring harness for a possible short to power supply, then go to Step 7.
No | Go to the next step.
5 | INSPECT REAR HO2S • Inspect the rear HO2S. (See REAR HEATED OXYGEN SENSOR (HO2S) INSPECTION.) • Is there any malfunction? | Yes | Replace the rear HO2S, then go to Step 7. (See REAR HEATED OXYGEN SENSOR (HO2S) REMOVAL/INSTALLATION.)
No | Go to the next step.
6 | INSPECT PCM CONNECTOR FOR POOR CONNECTION • Turn the ignition switch off. • Disconnect the PCM connector. • Inspect for poor connection (such as damaged/pulled-out pins, corrosion). • Is there any malfunction? | Yes | Repair or replace the terminal, then go to the next step.
No | Go to the next step.
7 | VERIFY TROUBLESHOOTING OF DTC P0138 COMPLETED • Make sure to reconnect all disconnected connectors. • Clear the DTC from the PCM memory using the WDS or equivalent. • Perform the DRIVE MODE 1 and 3. (See OBD DRIVE MODE.) • Is the PENDING CODE same as the DTC present? | Yes | Replace the PCM, then go to the next step. (See PCM REMOVAL/INSTALLATION.)
No | Go to the next step.
8 | VERIFY AFTER REPAIR PROCEDURE • Perform the "AFTER REPAIR PROCEDURE". (See AFTER REPAIR PROCEDURE.) • Are any DTCs present? | Yes | Go to the applicable DTC inspection. (See DTC TABLE.)
No | DTC troubleshooting completed.