#
LCD UNIT REMOVAL/INSTALLATION

BHE092066901W01

1. Disconnect the negative battery cable.

2. Remove the following parts:

  (1) Lower panel(See LOWER PANEL REMOVAL/INSTALLATION.)
  (2) Console(See CONSOLE REMOVAL/INSTALLATION.)
  (3) Center panel module(See CENTER PANEL MODULE REMOVAL/INSTALLATION.)
  (4) Center ventilator grille(See VENTILATOR GRILLE REMOVAL/INSTALLATION.)

3. Remove in the order indicated in the table.

1 | Screw
2 | LCD unit (See LCD Unit Removal Note.) (See LCD Unit Installation Note.)
3 | Connector

4. Install in the reverse order of removal.

## LCD Unit Removal Note

1. Pull the lower LCD unit outward, detach clip A from the dashboard, and then remove the LCD unit.

## LCD Unit Installation Note

1. Install the LCD unit by lightly pressing on the shaded part shown in the figure.

  Caution

  • Do not press on the folding part of the display when installing. This may cause an impact that could damage the open/closing gear of the display, causing it to not operate properly.