#
MAGNETIC CLUTCH ADJUSTMENT

BHE074061010W01

1. Measure the clearance around the entire circumference between the pressure plate and A/C compressor pulley using a feeler gauge.

2. Inspect the clearance.

  • If not within the specification, adjust the clearance by changing the shim (0.2 mm {0.008 in}, 0.5 mm {0.02 in}) or the number of shims.

  Standard clearance
  0.20-0.45 mm {0.008-0.017 in}