#
DTC INSPECTION (IMMOBILIZER SYSTEM)

BHE090201077W02

## Security Light

1. Turn the ignition switch to the ON position.

2. Verify the security light state.

  • If there is any malfunction:

  – After any malfunction is detected, the security light will function as follows for approx. 1 min.

  • DTC 16 and lower: Flashes
  • DTC 21 and higher: Illuminated

  • If there is no malfunction:

  – The security light illuminates for approx. 3 s and goes out.

3. When any malfunction has been detected, read DTCs via flashing patterns displayed after the security light flashes or is illuminated for approx. 1 min.

  • Perform troubleshooting according to the corresponding DTC inspection.

  Note

  • A verified DTC is flashed 10 times repeatedly by the security light.
  • If multiple DTCs are verified, the security light displays only the smallest DTC.

## WDS OR EQUIVALENT

1. Connect the WDS or equivalent to the DLC-2.

2. Verify if any DTCs are displayed.

  • If any DTCs are displayed, carry out troubleshooting according to the corresponding DTC inspection.

3. Disconnect the WDS or equivalent.