#
PARKING BRAKE LEVER REMOVAL/INSTALLATION

BHE041244300W03

1. Remove the propeller shaft. (See PROPELLER SHAFT REMOVAL/INSTALLATION.)

2. Remove the front console.

3. Remove in the order indicated in the table.

4. Install in the reverse order of removal.

5. After installation, inspect the parking brake stroke and adjust if necessary.

1 | Parking brake switch connector
2 | Adjusting nut
3 | Parking brake lever
4 | Parking brake switch
5 | Clip
6 | Rear parking brake cable
7 | Front parking brake cable