#
AIR CLEANER ELEMENT INSPECTION

BHE011301005W07

1. Remove the air hose. (See INTAKE-AIR SYSTEM REMOVAL/INSTALLATION.)

2. Unclip the air cleaner cover. (See INTAKE-AIR SYSTEM REMOVAL/INSTALLATION.)

3. Remove the air cleaner element. (See INTAKE-AIR SYSTEM REMOVAL/INSTALLATION.)

4. Inspect the following items:

  • If there is any abnormality, clean or replace the air cleaner element.

  – Has the replacement interval come?
  – Is the air cleaner element soiled, damaged, or bent?
  – Are the air cleaner case and the air cleaner element correctly sealed?
  – Is the correct air cleaner element installed?