#
EVAPORATIVE EMISSIONS (EVAP) CONTROL SYSTEM OUTLINE

BHE011601074T01

## Features

• A canister design has been adopted to prevent discharge of evaporative gas into the atmosphere.

• A duty solenoid (purge solenoid valve) has been adopted to provide optimum control according to engine conditions.

• For evaporative purge control, refer to ENGINE CONTROL SYSTEM, EVAPORATIVE PURGE CONTROL. (See EVAPORATIVE PURGE CONTROL OUTLINE, EVAPORATIVE PURGE CONTROL BLOCK DIAGRAM, EVAPORATIVE PURGE CONTROL OPERATION.)