#
NO.25 A/C DOES NOT CUT OFF UNDER WIDE OPEN THROTTLE CONDITIONS

BHE010300103W27

25 | A/C DOES NOT CUT OFF UNDER WIDE OPEN THROTTLE CONDITIONS.
--- | ---
DESCRIPTION | The A/C compressor magnetic clutch does not disengage under wide open throttle.
POSSIBLE CAUSE | • APP sensor malfunction • Loosely installed TP sensor

Diagnostic procedure

STEP | INSPECTION | RESULTS | ACTION
--- | --- | --- | ---
1 | Does the A/C compressor disengage when the A/C switch is turned off? | Yes | Go to the next step.
No | Go to the symptom troubleshooting "No.24 A/C is always on or A/C compressor runs continuously". (See NO.24 A/C IS ALWAYS ON OR A/C COMPRESSOR RUNS CONTINUOUSLY.)
2 | Connect the WDS or equivalent to the DLC-2. Retrieve any continuous memory, KOEO and KOER DTCs. Are there any DTCs displayed? | Yes | DTC is displayed: Go to the applicable DTC inspection. (See DTC TABLE.)
No | No DTC is displayed: Inspect the APP sensor for proper adjustment.
3 | Verify test results. • If normal, return to the diagnostic index to service any additional symptoms. • If the malfunction remains, inspect the related Service Information and perform the repair or diagnosis.