#
MANUAL TRANSMISSION SPECIFICATIONS [Y16M-D]

BHE050001030T05

Item | Specifications
--- | ---
Transmission type | Y16M-D
Transmission control | Floor-shift
Shift assist | Synchromesh
Gear ratio | 1GR | 3.760
2GR | 2.269
3GR | 1.645
4GR | 1.187
5GR | 1.000
6GR | 0.843
Reverse | 3.564
Oil | Grade | API service GL-4 or GL-5
Viscosity | All season | SAE 75W-90
Capacity (approx. quantity) | (L {US qt, lmp qt}) | 1.75 {1.85, 1.54}