#
REAR DOOR LOWER LATCH REMOVAL/INSTALLATION

BHE091458490W06

1. Remove the rear door lower trim. (See REAR DOOR LOWER TRIM REMOVAL/INSTALLATION.)

2. Remove the rear door upper trim. (See REAR DOOR UPPER TRIM REMOVAL/INSTALLATION.)

3. Remove the front seat belt retractor. (See FRONT SEAT BELT REMOVAL/INSTALLATION.)

4. Remove the rear door release handle. (See REAR DOOR RELEASE HANDLE REMOVAL/INSTALLATION.)

5. Detach the clip and disconnect the rear door lower latch switch connector.

6. Remove bolt A.

7. Remove bolts B, then remove the rear door lower latch.

8. Install in the reverse order of removal.

9. Adjust the door. (See DOOR ADJUSTMENT.)