#
SHIFT CONTROL OPERATION

BHE051318901T05

## Range determination

• Each range is determined by operating the selector lever, and switching on/off the switch in the TR switch internal circuit. The present range is detected according to the on/off signal of the switch.

• The following switches are built into the TR switch, and determine each range when the switch is on.

  P position switch
  R position switch
  N position switch
  D range switch