#
SECURITY LIGHT: 12, DTC B2103/P1260

BHE090201077W07

SECURITY LIGHT: 12 | Coil malfunction
DTC: B2103/P1260
DETECTION CONDITION | • Coil malfunction
POSSIBLE CAUSE | • Coil malfunction • Poor connection of the coil connector

## Diagnostic Procedure

STEP | INSPECTION | ACTION
--- | --- | ---
1 | INSPECT CONNECTOR CONNECTION • Are the coil connector and the keyless unit connector securely connected? | Yes | Replace the coil. (See COIL REMOVAL/INSTALLATION.)
No | Connect the connector securely.