#
DTC 00:ER10

BHE090266900W07

DTC 00:Er10 | Cassette deck-base unit communication line
DETECTION CONDITION | • Base unit detects communication error with cassette deck.
POSSIBLE CAUSE | • Malfunction of connectors between base unit and cassette deck • Cassette deck malfunction • Base unit malfunction

Diagnostic procedure

STEP | INSPECTION | ACTION
--- | --- | ---
1 | Remove the cassette deck and verify the connector condition (bent pins, poor female terminal connection, trapped foreign material) Is the connector normal? | Yes | Go to the next step.
No | Repair the connector and go to the next step.
2 | Assemble the cassette deck to the base unit and verify the assembly condition. Is the assembly condition normal? | Yes | Go to the next step.
No | Repair the assembly and go to the next step.
3 | Clear the DTC, turn the ignition switch to the ON position and then hold for 3 s or more. Is DTC 00: Er10 displayed? | Yes | Replace the base unit and cassette deck.
No | DTC troubleshooting completed.