#
TECHNICAL DATA

BHE055001029M01

Item | Specification
--- | ---
Transmission type | R15M-D
Engine type | 13B-MSP | 13B-Turbo | EXCEPT 13B-MSP, 13B-Turbo
Transmission oil | Type | API Service GL-4 or GL-5
Viscosity | All-season | SAE 75W-90
Above 10°C {50°F} | SAE 80W-90
Capacity | (L {US qt, lmp qt}) | 2.5 {2.6, 2.2} | 2.8 {3.0, 2.5}
Mainshaft runout | (mm {in}) | Maximum | 0.03 {0.0012}
Clearance between mainshaft and each gear | (mm {in}) | Maximum | 0.15 {0.006}
Clearance between reverse idler gear bushing and shaft | (mm {in}) | Standard | 0.02-0.05 {0.0008-0.0020}
Maximum | 0.15 {0.006}
Clearance between shift fork and clutch hub sleeve groove | (mm {in}) | Standard | 0.2-0.3 {0.008-0.012}
Maximum | 0.5 {0.020}
Clearance between shift rod end and control rod | (mm {in}) | Standard | 0.8 {0.031} or less
Synchronizer
Clearance between synchronizer ring and flank surface of gear | (mm {in}) | Standard | 1.5 {0.059}
Maximum | 0.8 {0.031}
Synchronizer key | (mm {in}) | Standard | 1st/ 2nd | Length | 17.0 {0.670} | 18.0 {0.709} | 17.0 {0.670}
Height | 4.7 {0.185} | 5.45 0.215} | 4.25 {0.167}
Width | 5.0 {0.197} | 6.0 {0.236} | 5.0 {0.197}
3rd/ 4th | Length | 17.0 {0.670}
Height | 4.25 {0.167}
Width | 5.0 {0.197}
5th/ reverse | Length | 17.0 {0.670}
Height | 4.25 {0.167}
Width | 5.0 {0.197}
Clearance between C-clip and mainshaft groove | (mm {in}) | Standard | 0-0.1 {0-0.004}
C-clip | (mm {in}) | Thickness | 2.9, 3.0, 3.1 {0.114, 0.118, 0.122}
Clearance between the thrust lock washer and C-clip (5th gear end play) | (mm {in}) | Standard | 0.1-0.2 {0.004-0.008}
Thrust lock washer | (mm {in}) | Thickness | 6.2, 6.3, 6.4, 6.5, 6.6, 6.7 {0.244, 0.248, 0.252, 0.256, 0.260, 0.264}
End play
Clutch housing | (mm {in}) | Standard | 0-0.1 {0-0.004}
Adjustment shim | 0.3, 0.4, 0.5, 0.6, 0.7 {0.012, 0.016, 0.020, 0.024, 0.028}
Mainshaft front bearing | (mm {in}) | Standard | 0-0.05 {0-0.002}
Adjustment shim | 0.1, 0.3 {0.004, 0.012}
Countershaft front bearing | (mm {in}) | Standard | 0-0.1 {0-0.004}
Adjustment shim | 0.1, 0.3 {0.004, 0.012}
Clearance between synchronizer key (clutch hub) and synchronizer ring | (mm {in}) | Standard | 0.66-2.0 {0.026-0.079}
Thrust washer (1st) | (mm {in}) | Thickness | 2.5, 3.0, 3.5 {0.098, 0.118, 0.138}
Detent ball spring free length | (mm {in}) | Standard | 22.5 {0.886}
5th/reverse rataining spring free length | (mm {in}) | Standard | 73.0 {2.874}
Select lock spindle spring free length | (mm {in}) | Standard | 75.1 | 43.25 | -