#
CONTROLLER AREA NETWORK (CAN) SYSTEM WIRING DIAGRAM

BHE014000140T52

• The PCM performs communication of vehicle information with the EPS control module, TCM (AT), keyless unit, instrument cluster, DSC HU/CM, Steering angle sensor and DLC-2.

1 | PCM
2 | EPS control module
3 | AT
4 | TCM
5 | Steering angle sensor
6 | Twisted pair
7 | DSC HU/CM
8 | Keyless unit
9 | DLC-2
10 | Instrument cluster
11 | CAN_H
12 | CAN_L