#
FUEL GAUGE SENDER UNIT INSPECTION

BHE092260960W02

## Fuel Gauge Sender Unit (Main)

1. Move the float to the topmost and bottommost positions, and verify that the resistance between terminals A and B of the fuel gauge sender unit (main) and the position of the float are as shown in the figure.

  • If they are not as shown in the figure, replace the fuel gauge sender unit (main).

## Fuel Gauge Sender Unit (Sub)

1. Move the float to the topmost and bottommost positions, and verify that the resistance between terminals A and B of the fuel gauge sender unit (sub) and the position of the float are as shown in the figure.

  • If they are not as shown in the figure, replace the fuel gauge sender unit (sub).