#
FRONT BUMPER REMOVAL/INSTALLATION

BHE091050010W01

1. Disconnect the negative battery cable.

2. Disconnect the front fog light connectors for vehicles with front fog lights.

3. Remove the front side turn lights. (See FRONT SIDE TURN LIGHT REMOVAL/INSTALLATION.)

4. Remove in the order indicated in the table.

1 | Fastener A
2 | Seal plate
3 | Screw A
4 | Screw B
5 | Fastener B
6 | Bolt
7 | Front bumper (See Front Bumper Removal Note.) (See Front Bumper Installation Note.)

5. Disconnect the headlight cleaner hose for vehicles with the headlight cleaner.

6. Install in the reverse order of removal.

7. Adjust the front fog light aiming for vehicles with the front fog lights. (See FRONT FOG LIGHT AIMING.)

## Front Bumper Removal Note

1. Pull the front bumper ends (wheel arch) outward to detach from the bumper slider.

  Caution

  • When detaching the front bumper from the bumper slider, the front bumper could fall and be damaged. Secure the front bumper so that it does not fall.

2. Remove the front bumper from the body.

## Front Bumper Installation Note

1. Spread the front bumper ends apart.

2. Attach the front bumper to the body.

3. Press the front bumper connecting area into the body to engage with the bumper slider.