#
A/C AMPLIFIER FUNCTION [FULL-AUTO AIR CONDITIONER]

BHE074061480T10

## Control List

• Function is based on five basic control items and two supplementary function items.

Basic control | Control content | Correction control
--- | --- | ---
Airflow temperature control | Airflow temperature automatic control | • Air mix actuator opening angle correction • MAX HOT and MAX COLD correction
Airflow volume control | Airflow volume automatic control | • Mild start correction • Warm-up correction • MAX HOT and MAX COLD correction • Defroster correction • Ambient temperature • Burn prevention function at start
Airflow volume manual control | • Defroster correction • Burn prevention at start function
Airflow mode control | Airflow mode automatic control | • Warm-up correction • MAX HOT and MAX COLD correction
Airflow mode manual control |
Air intake control | Air intake automatic control | • Defroster correction • MAX HOT and MAX COLD correction
Air intake manual control | • Defroster correction
A/C compressor control | A/C compressor automatic control | • Defroster correction • Ambient correction (during FRESH mode) • MAX HOT and MAX COLD correction
A/C compressor manual control | • Defroster correction

Supplemental functions
Fail-safe function
On-board function

## Control Transition Based on Switch Operation

Airflow temperature control, airflow volume control

Operation switch | Airflow temperature control | Airflow volume control
--- | --- | ---
Control prior to switch operation | Control prior to switch operation
Automatic control | Automatic control | Automatic control (Defroster correction) | Manual control
Fan switch | UP | Automatic control | Manual control*2 | Manual control*2 | Manual control
DOWN | Automatic control | Manual control*3 | Manual control*3 | Manual control
Airflow mode selector switch | Automatic control | Automatic control | Condition prior to operation | No change
Defroster | Automatic control | Defroster correction | Condition prior to operation | Automatic control (Defroster correction)
A/C switch | Automatic control | Automatic control | No change | No change
REC/FRESH switch | Automatic control | Automatic control | No change | No change
Temperature control dial | 18 (left end) | MAX COLD | MAX HI | MAX HI | No change
19-31 | Automatic control | Automatic control | No change | No change
32 (right end) | MAX HOT | AUTO HI*1 | AUTO HI | No change

  *1 :
Warm-up correction prioritized
  *2 :
Increases airflow to a level closer to current condition
  *3 :
Decreases airflow to a level closer to current condition

Airflow mode control, air intake control, A/C compressor control

Operation switch | Airflow mode control | Air intake control | A/C compressor control
--- | --- | --- | ---
Control prior to switch operation | Control prior to switch operation | Control prior to switch operation
Automatic control | Manual control | Automatic control | Manual control | Automatic control | Manual control
Fan switch | UP | Automatic control | No change | No change | No change | Automatic control | No change
DOWN | Automatic control | No change | No change | No change | Automatic control | No change
Airflow mode selector switch | Manual control | Manual control | Manual control*2 | No change | Manual control*3 | No change*3
Defroster switch | DEFROSTER | DEFROSTER | Defroster correction | Defroster correction | Defroster correction | Defroster correction
A/C switch | Automatic control | No change | Automatic control | No change | Manual control | Manual control
REC/FRESH switch | Automatic control | No change | Manual control | Manual control | Automatic control | No change
Temperature control dial | 18 (left end) | Automatic control | No change | Automatic control | No change | Automatic control | No change
19-31 | Automatic control | No change | Automatic control | No change | Automatic control | No change
32 (right end) | Automatic control | No change | Automatic control | No change | Automatic control | No change

  *1 :
Warm-up correction prioritized
  *2 :
If operated during defroster mode, returns to condition prior to defroster selection. However, if the REC/FRESH switch is operated during defroster mode, there is no change.
  *3 :
If operated during defroster mode, returns to condition prior to defroster selection. However, if the A/C switch is operated during defroster mode, there is no change.