#
LCD UNIT CONSTRUCTION

BHE092066901T02

## Structural View

• Located at the center of the dashboard.

1 | LCD unit

## Terminal Layout and Signal

Terminal | Signal
--- | ---
24-pin connector
| 1A | Video (B)
1B | Video (G)
1C | Video (composite sync)
1D | Video (R)
1E | Video GND
1F | Video GND
1G | Shield GND
1H | -
1I | Monitor serial output
1J | -
1K | Monitor serial input
1L | -
1M | Control illumination
1N | -
1O | ACC
1P | GND
1Q | B+
1R | Parking brake signal
1S | Shield GND
1T | R range signal
1U | UART2
1V | Illumination
1W | UART1
1X | -

Terminal | Signal
--- | ---
6-pin connector
| 2A | Power
2B | GND
2C | Illumination
2D | -
2E | Shield GND
2F | -