#
FUEL-FILLER LID ADJUSTMENT

BHE091042410W02

1. Measure the gap and height difference between the fuel-filler lid and the body.

2. Loosen the fuel-filler lid installation bolts, and adjust the fuel-filler lid.

  Standard clearance
  a: 1.7-3.7 mm {0.07-0.14 in}
  b: -0.5-1.5 mm {-0.01-0.05 in}
  c: -1.0-1.0 mm {-0.03-0.03 in}
  d: 1.8-3.8 mm {0.08-0.14 in}
  e: 1.7-3.7 mm {0.07-0.14 in}
  f: -0.8-1.2 mm {-0.03-0.04 in}

3. Tighten the bolts.