#
FRONT DOOR SPEAKER INSPECTION

BHE092066961W02

1. Verify the resistance between front door speaker terminals.

  • If the resistance is not within the specification, replace the front door speaker.

  Resistance
  Standard: 4 ohms
  BOSE: 0.5 ohms

2. Connect a 1.5 V battery to the front door speaker and verify that noise is sound from the front door speaker.

  • If no sound is output, replace the front door speaker.