#
BLOWER UNIT REMOVAL/INSTALLATION

BHE071161140W01

1. Disconnect the negative battery cable.

2. Remove the following parts:

  1. Ashtray
  2. Console (See CONSOLE REMOVAL/INSTALLATION.)
  3. Glove compartment (See GLOVE COMPARTMENT REMOVAL/INSTALLATION.)
  4. Side panel (See SIDE PANEL REMOVAL/INSTALLATION.)
  5. Lower panel (See LOWER PANEL REMOVAL/INSTALLATION.)
  6. Column cover (See COLUMN COVER REMOVAL/INSTALLATION.)
  7. Steering shaft installation nuts (See STEERING WHEEL AND COLUMN REMOVAL/INSTALLATION.)
  8. A-pillar trim (See A-PILLAR TRIM REMOVAL/INSTALLATION.)
  9. Dashboard (See DASHBOARD REMOVAL/INSTALLATION.)

3. Remove the A/C unit from the dashboard.

4. Remove the blower unit as shown in the figure.

5. Install in the reverse order of removal.