#
INSTRUMENT CLUSTER SPECIFICATIONS

BHE092255430T02

Item | Specification
--- | ---
Speedometer | Meter type | LCD
Indication range | (mph {km/h}) | 0-186 {0-299}
Input signal communication system | CAN system
Input signal source | DSC HU/CM
Rated voltage | (V) | DC 12
Tachometer | Meter type | Stepping motor type
Indication range | (rpm) | 0-10,000 (13B-MSP (High Power)) 0-9,000 (13B-MSP (Standard Power))
Red zone | (rpm) | 9,000-10,000 (13B-MSP (High Power)) 7,500-9,000 (13B-MSP (Standard Power))
Input signal communication system | CAN system
Input signal source | PCM
Rated voltage | (V) | DC 12
Fuel gauge | Meter type | Stepping motor type (Reset-to-zero type)
Input signal communication system | Conventional communication system
Input signal source | Fuel gauge sender unit
Rated voltage | (V) | DC 12
Water temperature gauge | Meter type | Stepping motor type (Medium range stabilized type)
Input signal communication system | CAN system
Input signal source | PCM
Rated voltage | (V) | DC 12
Odometer/Tripmeter | Display | LCD
Indication digits | Odometer: 6 digits, Tripmeter: 4 digits
Input signal communication system | CAN system
Input signal source | PCM
Rated voltage | (V) | DC 12
Warning alarms | Sound frequency | (Hz) | 800-1,500
Output sound pressure level | (dB) | 75.0 (over-revolution warning alarm) 67.5 (except over-revolution warning alarm)
Lights-on reminder warning alarm | Sound frequency | (Hz) | 1,000
Sound cycle |
Key reminder warning alarm | Sound frequency | (Hz) | 800
Sound cycle |
Over-revolution warning alarm | Sound frequency | (Hz) | 1,500
Sound cycle |
Seat belt warning alarm | Sound frequency | (Hz) | 800
Sound cycle |