#
DRIVE BELT ADJUSTMENT

BHE011015800W02

## Generator Drive Belt

1. Remove the engine cover. (SeeENGINE COVER REMOVAL/INSTALLATION.)

2. Loosen generator installation bolt A and locknut B.

3. Adjust the drive belt deflection and tension by turning adjusting bolt C to the specification.

  Drive belt deflection (with pressure of 98 N {10 kgf, 22 lbf})
  4.5-5.0 mm {0.18-0.19 in}
  Drive belt tension (when using the SST)
  519-666 N {53.0-67.9 kgf, 117-149 lbf}

4. Tighten generator installation bolt A and locknut B to the specified torque.

  Tightening torque
  A: 38-51 N·m {3.9-5.2 kgf·m, 29-37 ft·lbf}
  B: 20-30 N·m {2.1-3.0 kgf·m, 15-22 ft·lbf}

5. Crank the engine and measure the deflection and tension again. If not within the specification, repeat from Step 2 again.

6. Install the engine cover. (SeeENGINE COVER REMOVAL/INSTALLATION.)

## A/C Drive Belt

1. Remove the engine cover. (SeeENGINE COVER REMOVAL/INSTALLATION.)

2. Loosen idle pulley locknut A.

3. Adjust the drive belt deflection and tension by turning adjusting bolt B to the specification.

  Drive belt deflection (with pressure of 98 N {10 kgf, 22 lbf})
  3.3-4.0 mm {0.13-0.15 in}
  Drive belt tension (when using the SST)
  519-617 N {53.0-62.9 kgf, 117-138 lbf}

4. Tighten idle pulley locknut A to the specified torque.

  Tightening torque
  37.2-51.9 N·m {3.80-5.29 kgf·m, 27.5-38.2 ft·lbf}

5. Crank the engine and measure the deflection and tension again. If not within the specification, repeat from Step 2 again.

6. Install the engine cover. (SeeENGINE COVER REMOVAL/INSTALLATION.)