#
BRAKE PEDAL REMOVAL/INSTALLATION

BHE041143300W02

  Caution

  • If the brake switch is removed from the brake pedal or interlock cable, its proper functioning cannot be guaranteed when reinstalled. Therefore, replace the brake switch with a new one if it is removed.
  • When replacing the brake pedal (AT), it is possible that the installation of the interlock cable could become defective. Always refer to the interlock cable installation note when replacing the brake pedal. (See Interlock Cable Installation Note.)

  Note

  • When the brake switch connector is connected to the brake switch, the clearance between the pedal and the brake switch is adjusted automatically. However, this mechanism will only function one time.

1. Remove in the order indicated in the table.

2. Install in the reverse order of removal.

1 | Brake switch connector (See Brake Switch Connector Installation Note.)
2 | Snap pin
3 | Clevis pin
4 | Brake switch (See Brake Switch Installation Note.)
5 | Interlock cable (AT) (See Interlock Cable Installation Note.)
6 | Brake pedal
7 | Pedal pad

## Brake Switch Installation Note

1. Install the new brake switch to the brake pedal (MT) or the interlock cable (AT), and secure it by turning it clockwise 45° (AT) or counterclockwise 45° (MT).

## Brake Switch Connector Installation Note

1. Inspect the brake pedal. (See BRAKE PEDAL INSPECTION.)

2. With the brake pedal in its original position, install the brake switch to the brake switch connector.