#
REAR DOOR LOCK STRIKER REMOVAL/INSTALLATION

BHE091458490W09

## Upper

1. Remove the following parts:

  (1) A-pillar trim (SeeA-PILLAR TRIM REMOVAL/INSTALLATION.)
  (2) Sunvisor (See SUNVISOR REMOVAL/INSTALLATION.)
  (3) Assist handle (See ASSIST HANDLE REMOVAL/INSTALLATION.)
  (4) Roof side trim (See ROOF SIDE TRIM REMOVAL/INSTALLATION.)
  (5) Inner scuff plate (See INNER SCUFF PLATE REMOVAL/INSTALLATION.)
  (6) Rear seat (See REAR SEAT REMOVAL/INSTALLATION.)
  (7) Tire house trim (See TIRE HOUSE TRIM REMOVAL/INSTALLATION.)
  (8) Rear pillar trim (See REAR PILLAR TRIM REMOVAL/INSTALLATION.)
  (9) Interior light (See INTERIOR LIGHT REMOVAL/INSTALLATION.)
  (10)• Map light (See MAP LIGHT REMOVAL/INSTALLATION.)
  (11) Headliner (See HEADLINER REMOVAL/INSTALLATION.)

2. Remove the bolts A from the curtain air bag module.

3. Remove the bolt, then remove the bracket.

4. Remove the bolts, then remove the rear door lock striker (upper).

5. Install in the reverse order of removal.

6. Adjust the door. (See DOOR ADJUSTMENT.)

## Lower

1. Remove the outer scuff plate. (See OUTER SCUFF PLATE REMOVAL/INSTALLATION.)

2. Remove the screws, then remove the rear door lock striker (lower).

3. Install in the reverse order of removal.

4. Adjust the door. (See DOOR ADJUSTMENT.)