#
REAR TILT MOTOR INSPECTION

BHE091388651W01

1. Disconnect the rear tilt motor connector.

2. Connect battery positive voltage to rear tilt motor terminal A or B, then verify that the rear tilt motor operate as shown in the table.

  • If the rear tilt motor does not operate as indicated in the table, replace the rear tilt motor.

Motor operation | Connection
--- | ---
B+ | GND
Up | B | A
Down | A | B