#
SEAT BELT OUTLINE

BHE081157100T01

## Features

Improved safety | • Three-point seat belt with the following functions for front seat passengers adopted – ELR (Emergency Locking Retractor: emergency locking mechanism) – Pre-tensioner (See PRE-TENSIONER SEAT BELT CONSTRUCTION/OPERATION.) – Load limiter, which adjusts restraint force of the seat belt to reduce the possibility of injury to passengers caused by excess seat belt pressure after pre-tensioner operation – Seat belt lock release, which releases the lock on the front seat belt when the rear door is opened to prevent interference. • Three-point seat belt with the following functions for rear seat passengers adopted – ELR – ALR (Automatic Locking Retractor: child-restraint seat locking mechanism)