#
IGNITION KEY ILLUMINATION FUNCTION

BHE091851311T05

• The illumination time of the ignition key illumination is controlled by the microcomputer in the instrument cluster.

• The ignition key illumination glows when the ignition switch is at the LOCK or ACC position and any door is open.

1 | Key reminder switch
2 | Ignition key illumination bulb
3 | Instrument cluster
4 | And
5 | Timer
6 | Micro computer
7 | Door switch (Driver's side)