#
SUNROOF UNIT REMOVAL/INSTALLATION

BHE091569850W02

1. Disconnect the negative battery cable.

2. Remove the following parts:

  (1) Roof side trim (See ROOF SIDE TRIM REMOVAL/INSTALLATION.)
  (2) A-pillar trim (See A-PILLAR TRIM REMOVAL/INSTALLATION)
  (3) Rear seat (See REAR SEAT REMOVAL/INSTALLATION)
  (4) Inner scuff plate (See INNER SCUFF PLATE REMOVAL/INSTALLATION.)
  (5) Tire house trim (See TIRE HOUSE TRIM REMOVAL/INSTALLATION.)
  (6) Rear pillar trim (See REAR PILLAR TRIM REMOVAL/INSTALLATION.)
  (7) Map light (See MAP LIGHT REMOVAL/INSTALLATION.)
  (8) Interior light (See INTERIOR LIGHT REMOVAL/INSTALLATION.)
  (9) Sunvisor (See SUNVISOR REMOVAL/INSTALLATION.)
  (10) Assist handle (See ASSIST HANDLE REMOVAL/INSTALLATION.)
  (11) Headliner (See HEADLINER REMOVAL/INSTALLATION.)
  (12) Head impact pad (See HEAD IMPACT PAD REMOVAL/INSTALLATION.)
  (13) Glass panel (See GLASS PANEL REMOVAL/INSTALLATION.)

3. Disconnect the front and rear drain hoses from the sunroof frame.

4. Remove the bolts from curtain air bag module points A.

5. Remove the bolt, then remove the bracket.

6. Remove the rear door striker (upper) .

7. Remove the rear set bracket.

8. Remove the nuts and screws, then remove the sunroof unit.

9. Install in the reverse order of removal.

10. Adjust the glass panel. (See GLASS PANEL ADJUSTMENT.)