#
FRONT FRAME REAR UPPER INSTALLATION

BHE098053390B02

1. When installing new parts, position each part so that the section measurement aligns with the body dimension.

2. Drill holes for plug welds before installing new parts.

3. Weld the 18 locations indicated by (A) and install the front frame rear upper.

4. After temporarily installing new parts, make sure the related parts fit properly.

5. Plug the one weld location indicated by (B) when installing the torque box.