#
MASS AIR FLOW (MAF)/INTAKE AIR TEMPERATURE (IAT) SENSOR REMOVAL/INSTALLATION

BHE014013215W01

1. Remove the MAF/IAT sensor connector.

2. Remove in the order indicated in the table.

1 | Screw (See Screw Installation Note.)
2 | MAF/IAT sensor (See Mass Air Flow (MAF)/Intake Air Temperature (IAT) Sensor Installation Note.)

3. Install in the reverse order of removal.

## Mass Air Flow (MAF)/Intake Air Temperature (IAT) Sensor Installation Note

1. Before installation of the MAF/IAT sensor, replace the O-ring.

## Screw Installation Note

1. After installation of the screws, verify that the MAF/IAT sensor is installed securely.