#
REAR CROSSMEMBER REMOVAL/INSTALLATION

BHE021428400W01

  Caution

  • Performing the following procedures without first removing the ABS wheel-speed sensor may possibly cause an open circuit in the wiring harness if it is pulled by mistake. Before operations, remove the ABS wheel-speed sensor (axle side) and move the sensor away from the harnesses.

1. Remove the exhaust pipe. (See EXHAUST SYSTEM REMOVAL/INSTALLATION.)

2. Remove the propeller shaft. (See PROPELLER SHAFT REMOVAL/INSTALLATION.)

3. Remove the power plant frame. (See Power Plant Frame Removal Note.) (See Power Plant Frame Removal Note.) (See Power Plant Frame Removal Note.) (See Power Plant Frame Installation Note.) (See Power Plant Frame Removal Note.) (See Power Plant Frame Installation Note.)

4. Remove the rear drive shaft. (See REAR DRIVE SHAFT REMOVAL/INSTALLATION.)

5. Remove the rear differential. (See REAR DIFFERENTIAL REMOVAL/INSTALLATION.)

6. Remove in the order indicated in the table.

7. Install in the reverse order of removal.

8. Inspect the rear wheel alignment. (See REAR WHEEL ALIGNMENT.)

1 | Rear stabilizer (See REAR STABILIZER REMOVAL/INSTALLATION.)
2 | Rear axle component (See Rear Axle Component Removal Note.)
3 | Stopper plate
4 | Parking brake cable
5 | Rear crossmember component (See Rear Crossmember Component Removal Note.)
6 | Rear trailing link (upper)
7 | Rear trailing link (lower)
8 | Rear lateral link (upper)
9 | Rear lateral link (lower)
10 | Toe control link
11 | Rear crossmember
12 | No.2 bushing (See No.2 Bushing Removal Note.) (See No.2 Bushing Installation Note.)
13 | No.3 bushing (See No.3 Bushing Removal Note.) (See No.3 Bushing Installation Note.)

## Rear Axle Component Removal Note

1. Support the knuckle using a jack.

2. Using the SST, disconnect the rear trailing link (upper) ball joint.

3. Remove the rear trailing link (lower) outer bolt.

4. Using the SST, disconnect the rear lateral link (upper) ball joint.

5. Using the SST, disconnect the rear lateral link (lower) ball joint.

6. Remove the toe control link outer bolt.

7. Remove the shock absorber lower bolt.

8. Remove the rear axle component.

## Rear Crossmember Component Removal Note

  Warning

  • Be sure that the crossmember component is securely supported by the jack. If not securely supported, the crossmember component could fall, resulting in serious injury or death, and damage to the vehicle.

1. Support the rear crossmember with the jack, and remove the bolt.

2. Remove the rear crossmember component.

## No.2 Bushing Removal Note

1. Mark the rear crossmember with the bushing hole aligned as shown in the figure.

2. Using the SST, remove the bushing.

## No.3 Bushing Removal Note

1. Mark the rear crossmember with the bushing hole aligned as shown in the figure.

2. Using the SST, remove the bushing.

## No.3 Bushing Installation Note

1. Install the new bushing according to the marking made during bushing removal.

2. Using the SST, press fit the bushing.

## No.2 Bushing Installation Note

1. Install the new bushing according to the marking made during bushing removal.

2. Using the SST, press fit the bushing.