#
INTERIOR LIGHTING SYSTEM CONTROL SYSTEM OPERATION

BHE091851311T04

Conditions before operation (Conditions which must be satisfied) | Operation condition | Interior light | Cancel condition (When any condition satisfied)
--- | --- | --- | ---
Illumination time | Brightness
• Turn the ignition switch to the LOCK or ACC position. • All doors are closed. (All door switches are off.) | Any door open. (Any door switch is on.) | Approx.5 min | 100 % | • All doors are closed. (Any door switch is off.) • After illumination time.*1
• Key extracted from steering lock. (Key reminder switch is off.) • All doors are closed. (All door switches are off.) • Driver's door lock knob is locked. (Door lock-link switch is in lock position.) | Driver's door lock knob is unlocked. (Door lock-link switch is in unlock position.) | Approx.30 s | 100 % | • Turn the ignition switch to the ON position. • Any door open. (Any door switch is on.) • Driver's door lock knob is locked. (Door lock-link switch is in lock position.) • After illumination time.*1
• Key inserted into steering lock. (Key reminder switch is on.) • All doors are closed. (All door switches are off.) | Key extracted from steering lock. (Key reminder switch is off.) | Approx.15 s | 100 % | • Turn the ignition switch to the ON position. • Driver's door lock knob is locked. (Door lock-link switch is in lock position.) • After illumination time.*1
• Turn the ignition switch to the LOCK or ACC position. • Any door open. (Any door switch is on.) • Driver's door lock knob is unlocked. (Door lock-link switch is in unlock position.) | All doors are closed. (All door switches are off.) | Approx.15 s | 60 % | • Turn the ignition switch to the ON position. • Any door open. (Any door switch is on.) • Driver's door lock knob is locked. (Door lock-link switch is in lock position.) • After illumination time.*1

  *1 :
After interior light is turned off according to this cancel condition, the light will illuminate again when either of the following conditions are satisfied

• After all doors are closed, then any door is reopened. (After All door switches are off, any door switch is on.)

• Ignition switch is at the ON position. (IG on.)

1 | Door lock-link switch
2 | Door switch
3 | Key reminder switch
4 | IG 1
5 | Lock
6 | Unlock
7 | ON
8 | OFF
9 | View A
10 | Map light/Interior light/Courtesy light/Ground illumination light
11 | Approx. 30 S
12 | Approx. 15 S
13 | Approx. 1 S
14 | Approx. 5 Min