#
PCM CONFIGURATION

BHE014018880W03

1. Connect the WDS or equivalent to the DLC-2.

2. Set up the WDS or equivalent (including the vehicle recognition).

3. Select "Module Programming".

4. Select "Programmable Module Installation".

5. Select "PCM" and perform procedures according to directions on the WDS or equivalent screen.

  Note

  • If the PCM is replaced with a new one, the PCM stores DTC P0602 and illuminates the MIL even though no malfunction is detected. This means the PCM has not been configured yet.

6. Retrieve DTCs using the WDS or equivalent and verify that there is no DTC present.

  • If any DTC is present, perform applicable DTC inspection. (See DTC TABLE.)