#
REAR DOOR UPPER LATCH REMOVAL/INSTALLATION

BHE091458490W04

1. Remove the rear door lower trim. (See REAR DOOR LOWER TRIM REMOVAL/INSTALLATION.)

2. Remove the rear door upper trim. (See REAR DOOR UPPER TRIM REMOVAL/INSTALLATION.)

3. Remove clips A and B, and disconnect the rear door upper latch switch connector.

4. Remove the rear door upper latch cable from the release handle.

5. Remove the bolts, then remove the rear door upper latch.

6. Install in the reverse order of removal.