#
COMBINED SENSOR REMOVAL/INSTALLATION

BHE041543770W01

  Caution

  • The internal parts of the combined sensor could be damaged if dropped. Be careful not to drop the combined sensor. Replace the combined sensor if it is subjected to an impact. Also, do not use an impact wrench or other similar air tools when removing/installing the sensor.

1. Remove the rear console.

2. Remove in the order indicated in the table.

1 | Combined sensor connector
2 | Nut
3 | Combined sensor

3. Install in the reverse order of removal.

4. After installation, perform the combined sensor initialization procedure. (See COMBINED SENSOR INITIALIZATION PROCEDURE.)