#
DTC TABLE

BHE010200102W11
×: Applicable
-: Not applicable

DTC No. | Condition | MIL | DC | Monitor item | Memory function | Page
--- | --- | --- | --- | --- | --- | ---
P0030 | Front HO2S heater control circuit problem | ON | 2 | HO2S heater | × | (See DTC P0030)
P0031 | Front HO2S heater control circuit low | ON | 2 | HO2S heater | × | (See DTC P0031)
P0032 | Front HO2S heater control circuit high | ON | 2 | HO2S heater | × | (See DTC P0032)
P0037 | Rear HO2S heater control circuit low | ON | 2 | HO2S heater | × | (See DTC P0037)
P0038 | Rear HO2S heater control circuit high | ON | 2 | HO2S heater | × | (See DTC P0038)
P0076 | VDI solenoid valve control circuit low | OFF | 2 | CCM | × | (See DTC P0076)
P0077 | VDI solenoid valve control circuit high | OFF | 2 | CCM | × | (See DTC P0077)
P0101 | MAF sensor circuit range/performance problem | ON | 2 | CCM | × | (See DTC P0101)
P0102 | MAF sensor circuit low input | ON | 1 | CCM | × | (See DTC P0102)
P0103 | MAF sensor circuit high input | ON | 1 | CCM | × | (See DTC P0103)
P0107 | BARO sensor circuit low input | ON | 1 | CCM | × | (See DTC P0107)
P0108 | BARO sensor circuit high input | ON | 1 | CCM | × | (See DTC P0108)
P0111 | IAT sensor circuit range/performance problem | ON | 2 | CCM | × | (See DTC P0111)
P0112 | IAT sensor circuit low input | ON | 1 | CCM | × | (See DTC P0112)
P0113 | IAT sensor circuit high input | ON | 1 | CCM | × | (See DTC P0113)
P0117 | ECT sensor circuit low input | ON | 1 | CCM | × | (See DTC P0117)
P0118 | ECT sensor circuit high input | ON | 1 | CCM | × | (See DTC P0118)
P0122 | TP sensor No.1 circuit low input | ON | 1 | CCM | × | (See DTC P0122)
P0123 | TP sensor No.1 circuit high input | ON | 1 | CCM | × | (See DTC P0123)
P0125 | Insufficient coolant temperature for closed loop fuel control | ON | 2 | CCM | × | (See DTC P0125)
P0130 | Front HO2S circuit problem | ON | 2 | HO2S | × | (See DTC P0130)
P0131 | Front HO2S circuit low voltage | ON | 2 | HO2S | × | (See DTC P0131)
P0132 | Front HO2S circuit high voltage | ON | 2 | HO2S | × | (See DTC P0132)
P0133 | Front HO2S circuit slow response | ON | 2 | HO2S | × | (See DTC P0133)
P0138 | Rear HO2S circuit high voltage | ON | 2 | HO2S | × | (See DTC P0138)
P0139 | Rear HO2S circuit slow response | ON | 2 | HO2S | × | (See DTC P0139)
P0171 | System too lean | ON | 2 | Fuel system | × | (See DTC P0171)
P0172 | System too rich | ON | 2 | Fuel system | × | (See DTC P0172)
P0222 | TP sensor No.2 circuit low input | ON | 1 | CCM | × | (See DTC P0222)
P0223 | TP sensor No.2 circuit high input | ON | 1 | CCM | × | (See DTC P0223)
P0300 | Random misfire detected | Flash/ON | 1 or 2 | Misfire | × | (See DTC P0300)
P0301 | Front rotor misfire detected | Flash/ON | 1 or 2 | Misfire | × | (See DTC P0301, P0302)
P0302 | Rear rotor misfire detected | Flash/ON | 1 or 2 | Misfire | ×
P0327 | KS circuit low input | ON | 1 | CCM | × | (See DTC P0327)
P0328 | KS circuit high input | ON | 1 | CCM | × | (See DTC P0328)
P0335 | Eccentric shaft position sensor circuit problem | ON | 1 | CCM | × | (See DTC P0335)
P0336 | Eccentric shaft position sensor circuit range/performance problem | ON | 1 | CCM | × | (See DTC P0336)
P0410 | AIR system problem | ON | 2 | AIR system | × | (See DTC P0410)
P0420 | Catalyst system efficiency below threshold | ON | 2 | Catalyst | × | (See DTC P0420)
P0443 | Purge solenoid valve circuit problem | ON | 2 | CCM | × | (See DTC P0443)
P0461 | Fuel gauge sender unit circuit range/performance problem | ON | 2 | CCM | × | (See DTC P0461)
P0462 | Fuel gauge sender unit circuit low input | ON | 2 | CCM | × | (See DTC P0462)
P0463 | Fuel gauge sender unit circuit high input | ON | 2 | CCM | × | (See DTC P0463)
P0480 | Cooling fan No.1 control circuit problem | OFF | 2 | Other | × | (See DTC P0480)
P0481 | Cooling fan No.2 control circuit problem | OFF | 2 | Other | × | (See DTC P0481)
P0500 | VSS circuit problem | ON | 2 | CCM | × | (See DTC P0500)
P0505 | Idle air control system problem | OFF | - | - | - | (See DTC P0505)
P0562 | System voltage low (KAM) | ON | 1 | CCM | × | (See DTC P0562)
P0564 | Cruise control switch input circuit problem | OFF | 1 | Other | × | (See DTC P0564)
P0571 | Brake switch input circuit problem | OFF | 1 | Other | × | (See DTC P0571)
P0601 | PCM memory check sum error | ON | 1 | CCM | × | (See DTC P0601)
P0602 | PCM programming error | ON | 1 | CCM | × | (See DTC P0602)
P0604 | PCM random access memory error | ON | 1 | CCM | × | (See DTC P0604)
P0610 | PCM vehicle options error | ON | 1 | CCM | × | (See DTC P0610)
P0638 | Throttle actuator control circuit range/performance problem | ON | 1 | CCM | × | (See DTC P0638)
P0661 | SSV solenoid valve control circuit low | ON | 2 | CCM | × | (See DTC P0661)
P0662 | SSV solenoid valve control circuit high | ON | 2 | CCM | × | (See DTC P0662)
P0703 | Brake switch No.2 input circuit problem | ON | 2 | CCM | × | (See DTC P0703)
P0704 | CPP switch input circuit problem | ON | 2 | CCM | × | (See DTC P0704)
P0850 | Neutral switch input circuit problem | ON | 2 | CCM | × | (See DTC P0850)
P1260 | Immobilizer system problem | OFF | 1 | Other | - | (See DTC P1260)
P1574 | TP sensor output incongruent | ON | 1 | CCM | × | (See DTC P1574)
P1577 | APP sensor output incongruent | ON | 1 | CCM | × | (See DTC P1577)
P1686 | Metering oil pump control circuit low flow side problem | ON | 1 | Other | × | (See DTC P1686)
P1687 | Metering oil pump control circuit high flow side problem | ON | 1 | Other | × | (See DTC P1687)
P1688 | Metering oil pump control circuit initial check problem | ON | 1 | Other | × | (See DTC P1688)
P2006 | APV motor control circuit IC problem | ON | 2 | CCM | × | (See DTC P2006)
P2008 | APV motor control circuit/open | ON | 2 | CCM | × | (See DTC P2008)
P2096 | Target A/F feedback system too lean | ON | 2 | Fuel system | × | (See DTC P2096)
P2097 | Target A/F feedback system too rich | ON | 2 | Fuel system | × | (See DTC P2097)
P2101 | Drive-by-wire relay control circuit problem | ON | 1 | CCM | × | (See DTC P2101)
P2106 | Throttle actuator control system-forced limited power | ON | 1 | CCM | × | (See DTC P2106)
P2107 | Throttle actuator control module processor error | ON | 1 | CCM | × | (See DTC P2107)
P2108 | Throttle actuator control module performance error | ON | 1 | CCM | × | (See DTC P2108)
P2109 | TP sensor minimum stop range/performance problem | ON | 1 | CCM | × | (See DTC P2109)
P2112 | Throttle actuator control system range/performance problem | ON | 1 | CCM | × | (See DTC P2112)
P2119 | Throttle actuator control throttle body range/performance problem | ON | 2 | CCM | × | (See DTC P2119)
P2122 | APP sensor No.1 circuit low input | ON | 1 | CCM | × | (See DTC P2122)
P2123 | APP sensor No.1 circuit high input | ON | 1 | CCM | × | (See DTC P2123)
P2127 | APP sensor No.2 circuit low input | ON | 1 | CCM | × | (See DTC P2127)
P2128 | APP sensor No.2 circuit high input | ON | 1 | CCM | × | (See DTC P2128)
P2135 | TP sensor No.1/No.2 voltage correlation problem | ON | 1 | CCM | × | (See DTC P2135)
P2136 | TP sensor No.1/No.3 voltage correlation problem | ON | 1 | CCM | × | (See DTC P2136)
P2138 | APP sensor No.1/No.2 voltage correlation problem | ON | 1 | CCM | × | (See DTC P2138)
P2195 | Front HO2S signal stuck lean | ON | 2 | HO2S | × | (See DTC P2195)
P2196 | Front HO2S signal stuck rich | ON | 2 | HO2S | × | (See DTC P2196)
P2257 | AIR pump relay control circuit low | ON | 2 | CCM | × | (See DTC P2257)
P2258 | AIR pump relay control circuit high | ON | 2 | CCM | × | (See DTC P2258)
P2259 | AIR solenoid valve control circuit low | ON | 2 | CCM | × | (See DTC P2259)
P2260 | AIR solenoid valve control circuit high | ON | 2 | CCM | × | (See DTC P2260)
P2270 | Rear HO2S signal stuck lean | ON | 2 | HO2S | × | (See DTC P2270)
P2271 | Rear HO2S signal stuck rich | ON | 2 | HO2S | × | (See DTC P2271)
P2502 | Charging system voltage problem | OFF | 1 | Other | × | (See DTC P2502)
P2503 | Charging system voltage low | OFF | 1 | Other | × | (See DTC P2503)
P2504 | Charging system voltage high | OFF | 1 | Other | × | (See DTC P2504)
U0073 | CAN system communication error | (See DTC TABLE [MULTIPLEX COMMUNICATION SYSTEM])
U0101 | Communication error to TCM | (See DTC TABLE [MULTIPLEX COMMUNICATION SYSTEM])
U0121 | Communication error to ABS HU/CM | (See DTC TABLE [MULTIPLEX COMMUNICATION SYSTEM])
U0155 | Communication error to instrument cluster | (See DTC TABLE [MULTIPLEX COMMUNICATION SYSTEM])
U0167 | Communication error to keyless control module | (See DTC TABLE [MULTIPLEX COMMUNICATION SYSTEM])