#
CLIMATE CONTROL UNIT REMOVAL/INSTALLATION

BHE074061190W01

1. Disconnect the negative battery cable.

2. Remove the lower panel. (See LOWER PANEL REMOVAL/INSTALLATION.)

3. Remove the console. (See CONSOLE REMOVAL/INSTALLATION.)

4. Remove the center panel module. (See CENTER PANEL MODULE REMOVAL/INSTALLATION.)

5. Remove the climate control unit from the center panel module.

6. Install in the reverse order of removal.