#
WINDSHIELD WASHER HOSE REMOVAL/INSTALLATION

BHE091967460W01

1. Remove the windshield wiper arm and blade. (See WINDSHIELD WIPER ARM AND BLADE REMOVAL/INSTALLATION.)

2. Disconnect joint pipe A, then remove windshield washer hose A from clip A.

3. Remove the cowl grille. (See COWL GRILLE REMOVAL/INSTALLATION.)

4. Remove clips B.

5. Disconnect joint pipe B, then remove windshield washer hose A.

6. Disconnect windshield washer hose B from the washer nozzle, then remove windshield washer hose B.

7. Disconnect joint pipe C, then remove windshield washer hose C.

8. Remove windshield washer hose D from clips C.

9. Disconnect windshield washer hose D from the washer nozzle, then remove windshield washer hose D.

10. Install in the reverse order of removal.