#
WINDSHIELD WASHER MOTOR INSPECTION

BHE091976670W02

1. Disconnect the negative battery cable.

2. Remove the windshield washer tank. (See WINDSHIELD WASHER TANK REMOVAL/INSTALLATION.)

3. Connect battery positive voltage to windshield washer motor terminal A and terminal B to ground.

4. Verify that the windshield washer motor operates normally.

  • If there is any malfunction, replace the windshield washer motor.