#
AFTER REPAIR PROCEDURE [RC4A-EL]

BHE050201026W04

  Caution

  • After repairing a malfunction, perform the following procedure to verify that the malfunction has been corrected.
  • When performing this procedure, be sure to drive the vehicle at lawful speed and pay attention to the other vehicles.

1. Connect the WDS or equivalent to the DLC-2.

2. Turn the ignition switch to the ON position (engine off).

3. Select the clear code function and clear the DTC.

4. Perform the following DTC inspections to ensure that the DTCs have been resolved:

  • For P0705

  i. Start the engine.
  ii. Warm up the engine to normal operating temperature.
  iii. Depress the brake pedal, and shift the selector lever between P to D for 12 s or more.
  iv. Go to Step 5.

  • For P0706

  i. Start the engine.
  ii. Warm up the engine to normal operating temperature.
  iii. Depress the brake pedal, and shift the selector lever between P to D for 100 s or more.
  iv. Go to Step 5.

  • For P0707

  i. Start the engine.
  ii. Warm up the engine to normal operating temperature.
  iii. Drive the vehicle in M range, and shift the selector lever (operate up and down switches) between 1GR to 4 GR for 10 s or more.
  iv. Go to Step 5.

  • For P0708

  i. Start the engine.
  ii. Warm up the engine to normal operating temperature.
  iii. Drive the vehicle in M range, and push the steering shift switch between 1GR to 4GR for 10 s or more.
  iv. Go to Step 5.

  • For P0712

  i. Start the engine.
  ii. Warm up the engine to normal operating temperature.
  iii. Drive the vehicle in D range for 150 s or more.
  iv. Go to Step 5.

  • For P0713

  i. Start the engine.
  ii. Warm up the engine to normal operating temperature.
  iii. Drive the vehicle in D range at 20 km/h {12.4 mph} or more for 150 s or more.
  iv. Go to Step 5.

  • For P0715

  i. Start the engine.
  ii. Warm up the engine to normal operating temperature.
  iii. Drive the vehicle in D range at 40 km/h {25 mph} or more for 2 s or more.
  iv. Go to Step 5.

  • For P0720

  i. Start the engine.
  ii. Warm up the engine to normal operating temperature.
  iii. Drive the vehicle in D range, at 5 km/h {3 mph} or more for 3.5 s or more.
  iv. Go to Step 5.

  • For P0731, P0732

  i. Start the engine.
  ii. Warm up the engine to normal operating temperature.
  iii. Drive the vehicle in D range, at 10 km/h {6 mph} or more for 2 s or more.
  iv. Go to Step 5.

  • For P0733

  i. Start the engine.
  ii. Warm up the engine to normal operating temperature.
  iii. Drive the vehicle in D range, at 20 km/h {12 mph} or more for 2 s or more.
  iv. Go to Step 5.

  • For P0734

  i. Start the engine.
  ii. Warm up the engine to normal operating temperature.
  iii. Drive the vehicle in D range, at 40 km/h {25 mph} or more for 2 s or more.
  iv. Go to Step 5.

  • For P0743, P0748, P0753, P0758, P0763, P0768, P0743, P0841, P0846, P0871, P0960, P1759, P1764, U0073, U0100

  i. Start the engine.
  ii. Warm up the engine to normal operating temperature.
  iii. Drive the vehicle in D range and make sure that the gears shift smoothly from 1GR to 4GR.
  iv. Go to Step 5.

5. Gradually slow down and stop the vehicle.

6. Make sure that the repaired DTC does not recur.