#
TECHNICAL DATA

BHE055001029101

Item | Specification
--- | ---
Engine type | BP | 13B-MSP
Transmission oil | Type | API Service GL-4 or GL-5
Viscosity | All-season | SAE 75W-90
Capacity | (L {US qt, lmp qt}) | 1.75 {1.85, 1.54}
Drive gear thrust clearance | (mm {in}) | 1st | 0.15-0.40 {0.006-0.015}
2nd | 0.10-0.45 {0.004-0.017}
3rd | 0.10-0.35 {0.004-0.013}
4th | 0.10-0.35 {0.004-0.013}
6th | 0.10-0.40 {0.004-0.015}
Reverse | 0.10-0.45 {0.004-0.017}
Drive gear radial clearance | (mm {in}) | 1st | 0.015-0.066 {0.0006-0.0025}
2nd | 0.015-0.066 {0.0006-0.0025}
3rd | 0.015-0.068 {0.0006-0.0026}
4th | 0.065-0.115 {0.0026-0.0045}
5th (drive gear) | 0.029-0.072 {0.0012-0.0028}
6th | 0.015-0.068 {0.0006-0.0026}
Reverse | 0.015-0.066 {0.0006-0.0025}
Reverse idler gear radial clearance | (mm {in}) | 0.040-0.082 {0.0016-0.0032}
Clearance between synchronizer ring and flank surface of gear | (mm {in}) | 1st, 2nd, 3rd | Inner ring | 0.98-1.62 {0.04-0.06}
Middle ring | 0.68-1.92 {0.03-0.07}
Synchronizer ring | - | 0.88-1.72 {0.04-0.06}
3rd | 0.90-1.70 {0.04-0.06} | -
4th, 5th | 0.80-1.60 {0.04-0.06}
6th, Reverse | 0.88-1.52 {0.04-0.05}
Mainshaft maximum runout | (mm {in}) | 0.03 {0.0012}
Countershaft maximum runout | (mm {in}) | 0.03 {0.0012}
Clearance between clutch hub sleeve and shift fork | (mm {in}) | 0.15-0.35 {0.006-0.013}
Clearance between 4th gear inner race and thrust washer | (mm {in}) | 0-0.1 {0-0.0039}
Clearance between counter drive gear and snap ring | (mm {in}) | 0-0.1 {0-0.0039}
Clearance between roller bearing (countershaft) and snap ring | (mm {in}) | 0-0.1 {0-0.0039}
Clearance between bearing (main drive gear) and snap ring | (mm {in}) | 0-0.1 {0-0.0039}
Clearance between clutch hub component (5th/reverse) and snap ring | (mm {in}) | 0-0.1 {0-0.0039}
Clearance between 6th gear and snap ring | (mm {in}) | 0-0.11 {0-0.0043}
Clearance between clutch hub component (6th) and snap ring | (mm {in}) | 0-0.1 {0-0.0039}