#
FRONT DOOR CONSTRUCTION

BHE091158010T03

• The inner construction of the door, including the power window regulator, door speaker, door harness and other parts, have been integrated into a single door unit.

• Due to the integrated door unit, weight reduction has been achieved for the whole door.

• Waterproofing of the inner door unit parts is achieved due to sectional design.

• Fiberglass reinforced plastics have been adopted for the door unit carrier to improve rigidity.

• A ripple-shaped side impact bar has been adopted to improve rigidity in case of collision.

1 | Front door unit
2 | Front power window regulator
3 | Front power window motor
4 | Front door speaker
5 | Front door unit carrier
6 | Front door harness
7 | Side impact bar