#
TRIPLE SYNCHRONIZER MECHANISM STRUCTURE [Y16M-D]

BHE051101025T14

## Features

• A triple synchronizer mechanism is used for the first, second and third gears to improve synchromesh capacity.

• The triple synchronizer mechanism consists of a synchronizer ring, middle ring, and inner ring.

• The gear side inner surface of the inner ring can also be used as a friction surface in the triple synchronizer mechanism. This provides a stronger synchronization force compared to the double cone synchronizer mechanism and reduces operation force and meshing time.

## Structure

Structural view

1 | Synchronizer ring
2 | Middle ring
3 | Inner ring
4 | Hub sleeve
5 | Ball
6 | Synchronizer key
7 | Spring
8 | Clutch hub