#
HAZARD WARNING SWITCH INSPECTION

BHE091866401W01

1. Remove the console. (See CONSOLE REMOVAL/INSTALLATION.)

2. Remove the lower panel. (See LOWER PANEL REMOVAL/INSTALLATION.)

3. Remove the center panel module. (See CENTER PANEL MODULE REMOVAL/INSTALLATION.)

4. Verify that the continuity between the hazard switch terminals is as indicated in the table.

  • If not as indicated in the table, replace the center panel.